Titel: Verbindungen und Hocker
Warum diese Holzverbindung?

Bachelorarbeit von Namun Baek

Betreuende Lehrende: 
Jun-Prof. Dr. Thomas Pearce
Dipl.-Des. Timm Burkhardt

In meiner ersten Holzwerkkurs habe ich Holzklöppel von Hand gemacht, und dann habe ich gelernt, wie man Schwalbenschwanz- oder Zapfenverbindung usw. von Hand und Maschine herstellt. An Orten, wo man auf diese Weise Holzwerk lernen kann, lernt man meistens zum ersten Mal etwas über die Technik von Nut, Löchern und Zapfen in Holz. Tatsächlich kann man Holz einfach mit Schrauben oder Nägeln befestigen oder Möbel mit Dübel oder Domino zusammenbauen, und sie können viel schneller und einfacher arbeiten als traditionelle Holzverbindung, daher habe ich mich gefragt, warum man noch traditionelle Holzverbindung braucht zu lernen. Der Grund ist, dass traditionelle Holzverbindungen die auftretenden Kräfte (Druck-, Zug- und Scherkräfte etc.) möglichst so auf alle Teile übertragen und verteilen und die Leimfläche vergrößern. Auf diesen Grund ist traditionelle Holzverbindung stabiler.
Früher muss man zwar alle Prozesse vollständig von Hand arbeiten, aber heutzutage wird Holzverbindung auch maschinell hergestellt wie CNC. Und ich finde, dass es effizient ist, CNC zu verwenden, um Verbindung herzustellen, die schwer von Hand herzustellen sind. Während dieses Abschlusssemesters werde ich versuchen, verschiedene Holzverbindungen aus Korea und Deutschland mit CNC und von Hand herzustellen, die Vor- und Nachteile jeder Verbindungen zu analysieren und zu vergleichen. Schließlich habe ich vor, den Stuhl mit Verbindung zu bauen.

Title: Connections and stools
Why this wood connection?

Bachelor thesis by Namun Baek

Advisor: 
Jun-Prof. Dr. Thomas Pearce
Dipl.-Des. Timm Burkhardt

In my first woodworking class, I made wood billets by hand, and then I learned how to make dovetail joint, tenon joint, etc. by hand and machine. In places where you can learn woodwork in this way, you usually learn about the technique of groove, holes and tenons in wood for the first time. In fact, you can easily fasten wood with screws or nails or assemble furniture with dowels or dominoes, and they can work much faster and easier than traditional wood jointing, so I was wondering why you still need to learn traditional wood jointing. The reason is that traditional wood joint transmits and distributes the occurring forces (compressive, tensile, shear, etc.) to all parts as much as possible, and increases the gluing area. On this reason traditional wooden joint is more stable.
In the past, all processes have to be done completely by hand, but nowadays wood joining is also done by machines like CNC. And I find that it is efficient to use CNC to make joint which is hard to make by hand. During this final semester, I will try to make different wood joints from Korea and Germany with CNC and by hand, the advantages and disadvantages of each joint. 


Kontakt/Contact: 
Namun Baek
fprh63[at]gmail.com 

Foto von / photos by: Namun Baek

Alle Rechte liegen bei den Autor/innen der Arbeit.
All rights are reserved by the authors of the work.

